
			Major Projects in 2026, next year & years after		June 2026


Streets are 37 years old  (original 1989)	

		Asphalt Lifespan 	20-35 years

		Concrete Lifespan 	50-60 years


Roofs are 35 years old  (first 1991)

		Roof Underlayment Lifespan	      15-30 years  (asphalt underlayment)


2025 Costs:

Roof Replacement (Underlayment)			$1,617,000

Streets - Asphalt - Replace				   $448,550

Streets - Stamped Concrete - Entry - Replace	   $367,000

Buildings - Stucco & Wood Surfaces - Repaint	   $586,000

						Total:  $3,018,550    ($2,528,550 - Needed now per 2026 Reserve Study)


Sixteen (16) Other Major Projects:		Total:	   $772,500

					Grand Total:	$3,791,050



